
# USB Copier README


The idea ist o have a small rpi running and be able to attach a usb harddrive and when a second usb stick is attached it gets copied to the disk.

I also added a 16x2 LCD display to show the progress

# RPI Pinout



LCD Display 16x2 Pinout:



# USB Mount

Fix for newer Raspian Version:

This link <https://github.com/rbrito/usbmount/issues/2> has the solution.  
Edit /lib/systemd/system/systemd-udevd.service and change the line  
MountFlags=slave  
to  
MountFlags=shared  
then reboot